

PSTN or PBX TG:

Ivr Type = Prepaid calling card
Ivr Card Digit Length  = Variables
Disabled Voice Prompt 0
Ivr Preauthentication = 1
Ivr Language = None
MultiSession code: = **




Radius User:


host p 1.2.3.4
authenticationport p 1812
accountingport p 1813

host s 0.0.0.0
authenticationport s 1812
accountingport s 1813

retry = 3
timeout = 5
accountingtype = 2
billingvendor 1
sharedsecret ****


